국  문  규  격  서

Commodity Description

관    세

분류번호

정부물품

분류번호

품목번호

품명 및 규격서

단  위

수  량

HSK No.

GPCN No.

Item No.

Description

Unit

Q'ty

R710

2U Rack Server

EA

3

A. Feature

64bit Linux Cluster 3Node

- Processor : Intel Quad-Core  E5530  2.40GHz * 6EA

- Memory: 96GB DDR  667MHz ECC KIT (Max:430 GB)

- DDR3  18RDIMM or UDIMM Type

- 6CH RAID Controller

Raid 1+ Raid 5, PERC5/i Intergrated

- CDRW/DVD Combo Drive*3EA

- 870W Dual Power Supply*3EA

- 4Port 5708C Gigabit Ethernet*3EA

- 8slot SATA/SAS Drive Cage(Max:9TB SATA)

- Embedded ATI ES1000 with 16MB Memory

- Front control Panel: system chassis to provide user acess to

buttons,display   and I/O Interfaces

Form Factor	2U rack
Processors	Up to two quad-core Intel® Nehalem 5500 series standard or low-volt processors at up to 2.00GHz~2.93 GHz
Processor Sockets	2
Front Side Bus or HyperTransport	Intel QuickPath Interconnect(QPI) Maximum 6.GT/s
Cache	Intel Xeon 5500: 2x4 MB;
Chipset	Intel 5000X Tylersburg
Memory	Up to 144 GB (18 FBD DIMM slots): /1 GB/2 GB/4 GB/8 GB; DDR3 800 MHz Fully Buffered DIMMs (FBD) in matched pairs
I/O Slots	4 PCI slots: either PCIe riser with 4 PCI Express slots [one x16 or 2 PCI-X 64-bit/133 MHz and 1 PCI Express x8 slot
Drive Controller	SAS 6/iR, PERC 5/i or PERC 6/i
RAID Controller	Optional PERC integrated SAS/SATA daughtercard controller or adapter; PERC 6.2 Firmware
Drive Bays	3 hard drive base options: 8 x 2.5" Hard Drive Option: 2.5" HD Option: up to 8 SAS HDs (10 K); 4 x 3.5" Hard Drive Option: 3.5" HD Option: up to 4 SAS (10 K/15 K) or SATA (7.2 K) drives; 6 x 3.5" Hard Drive Option: 3.5" HD Option: up to 6 SAS (10 K/15 K) or SATA (7.2 K) drives; Peripheral bay options; Floppy Drive, DAT72 Tape Drive (not available with 6 x 3.5" hard drive base); Slim optical drive bay with choice of CD-ROM, VD-ROM or Combo CD-RW/DVD-ROM
Maximum Internal Storage	Up to 6TB: 6 x 1TB Nearline SAS (7.2k rpm)
Hard Drives1	2.5" SAS (10 K rpm): 36 GB, 73 GB, 146 GB, 147GB, 300GB 2.5" SAS (15 K rpm): 36 GB or 73 GB 3.5" SAS (10 K rpm): 146 GB, 300 GB, 400 GB 3.5" SAS (15 K rpm): 73 GB, 146 GB, 300 GB, 450 GB 3.5" SATA (7.2 K rpm): 160 GB, 250 GB, 500 GB, 750 GB, 1 TB 3.5" Nearline SAS (7.2k rpm): 500GB, 750GB, 1TB Mixed SAS/SATA supported in matched pairs
Network Interface Cards	Dual embedded Broadcom® NetXtreme II™ 5708 Gigabit Ethernet NIC with fail-over and load balancing. TOE (TCPIP Offload Engine) supported on Microsoft® Windows® Server™ 2003, SP1 or higher with Scalable Networking Pack. Supports many optional single-, dual-, or quad-port 10baseT, copper, or optical add-in NICs
Power Supply	Single or redundant 870W hot-plug auto-switching 110/220VAC or redundant hot plug -48-60V 20A DC power supplies . High energy efficiency power supplies are also available.
Video	Embedded ATI ES1000 with 16 MB memory
Remote Management	Baseboard Management Controller with IMPI 2.0 support; optional DRAC5 (advanced capabilities)
Operating Systems	Microsoft® Windows® Server Microsoft® Windows® Storage Server Red Hat & Cento Linux Novell® SUSE Linux

B. Consist of

C.ecification

64bit Linux Cluster

HANUL Software 2 Copy

- Intel.C.Compiler.version10.x for linux 64bit 1EA

- Intel.Fortran.Compiler.version10.x for linux 64bit 1EA

- Intel Cluster ToolKit V3.1(C++,Fortran,MLK,MPI)

- PGI.Compiler.version 6.x for linux 64bit 1EA

- mpich_kit for linux x86_64bit by PGI 6.x

- mpich1 for linux x86_64bit  by PGI 6.x

- NETCDF 3.6.x by PGI 6.x

- PBS Development Kit 1EA , ptools

- realvnc(remote management tool), tsclient

- ncftp ,hanul F/W(easy iptalbes)

- Nero.version 3.x for linux , True.Image.version 9.x for linux

- Hardware Software 3Y warranty,on-site within 4h response

. Accessories(H/W)

- OpenManage™

- third-party Versa rails, sliding rails, and cable management arm

- Category 5E Lan Cable

-SATA Storage

1TB SATA 7200RPM Disk(max15TB)

RAID 0, 1, 5, 10, 50을 통해 제공되는 향상된 성능 및 보호

PCI-X의 4배의 대역폭을 제공하는 동급 최고의 PCI Express 인터페이스

확장을 위한 12.0 Gbps의 넓은 외부 연결 포트는

연결 당 최대 3개의 MD1000 디스크 확장 엔클로져를 지원

일관성 확인 및 배경 패트롤 읽기 오류 보정 및 검출

원래 용량의 총 15TB를 제공하는 1 15 드라이브 엔클로저

PERC 5/E RAID 컨트롤러를 통해, 최대 3개의 엔클로져

45개의 드라이브 가 원래 용량의 최대 33.75TB에 대해 연결 당 1 데이지 체인

최대 15개인 1인치 x 3.5인치 SAS 핫플러그 3.0 Gbps 하드 드라이브,

10,000 또는 15,000 RPM 속도 조건

최대 15개인 1인치 x 3.5인치 SATA Ⅱ 핫플러그 3.0 Gbps 하드 드라이브

하드 드라이브, 7,200RPM 속도 조건

. Accessories(S/W)

-Library Install

grads v1&v2, ncarg v4&v5(PGI,INTEL,GCC Ver)

blas v3.x, Lapack v3.x,	gsview 3.6.x,,ncview 1.9.3c

vis5d+,	AAPP6, HDF4&5&EOS,,	fftw2&3

Scalapack,,Ferret,,IOAPI,,RIP4,lyx 1.x,IDL v7,Matlab R2009a

-Schedule Management

FreeNX, Remote GUI Tool,hanterm, Xmanager S/W

ncftp v3.2.0-1,	FTP Client S/W,ganglia v3.x

Cluster Resource Monitoring S/W

Openmanager v6.1, H/W management Tool

ncompress, APC Power Chute Business Edition

nmon

F. Remarks

Hard Ware 3yr Warranty & Software 3yr Warranty

( 하드웨어 3년 유지보수, 소프트웨어 3년 유지보수 )

4 hours response and Obstacle processing  solution